- 2K polling rate step added
- Minor bug fixes 
- Linux bug fixes

HOW TO UPDATE THE FIRMWARE ON YOUR M68 PRO WIRELESS, M64 PRO WIRELESS RECIVER: 

ALWAYS UPDATE DONGLE/RECIVER FIRST THEN MOUSE AFTER!

1. Connect the receiver to the computer using the USB cable, the update can be only be done on a pc.

2. Start the file: CherryXtrfyDongleFWUpdate. Press start.

3. Wait for the update to complete, it will automatically close the program when update finish.

4. Done! You can now go back to wireless and continue gaming.


如何更新M68 PRO无线、M64 PRO无线鼠标接收器上的固件：

1.使用USB电缆将鼠标接收器连接到计算机，固件只能在PC 上进行更新。

2.打开.cmd文件:接收器更新。更新将自动启动。

3.等待更新完成，更新完成后，后台会自动关闭程序。

4.完成！您现在可以返回无线模式，并继续游戏。

