- 2K polling rate step added
- Minor bug fixes 
- Linux bug fixes

HOW TO UPDATE THE FIRMWARE ON YOUR M68 PRO WIRELESS, M64 PRO WIRELESS RECIVER: 

ALWAYS UPDATE DONGLE/RECIVER FIRST THEN MOUSE AFTER!

1. Connect the mouse to the computer using the USB cable. Please ensure that the mouse is in wired mode, and the update can be only done on a pc.

2. Open the .exe file and press Start. 

3. Wait for the update to complete. When the software says "Update completed", press OK.

4. Done! You can now go back to wireless and continue gaming.


如何更新M68 PRO无线、M64 PRO无线鼠标上的固件：

1.使用USB电缆将鼠标连接到计算机。请确保鼠标处于有线模式，固件只能在PC 上进行更新。

2.打开.exe文件，然后点击“开始”。

3.等待更新完成，当软件显示“更新完成”时，点击OK。

4.完成！您现在可以返回无线模式，并继续游戏。

